

A



**ANANYA CHAKRAVARTHI SANGEETHA S**

**SANDEEP V PRAYAG SRIDHAR**

**1BM18EE007**

**1BM18EE045**

**1BM18EE068**

**1BM18EE041**

Final Year Project Report On

## “INTEGRATED SMART ENERGY METER WITH HOME AUTOMATION”

*Submitted in partial fulfillment of the requirements for the award of the Degree of Bachelor of Engineering*

*in*

***Electrical and Electronics Engineering***

Visvesvaraya Technological University, Belagavi

*Submitted by*

***Under the guidance of***

**Dr. S PRADEEPA**

Professor


**DEPARTMENT OF ELECTRICAL AND ELECTRONICS ENGINEERING**

### BMS COLLEGE OF ENGINEERING

**(Autonomous Institute, Affiliated to VTU)**

BULL TEMPLE ROAD, BENGALURU-560019

**2021-2022**



**BMS COLLEGE OF ENGINEERING**

**(Autonomous Institute, Affiliated to VTU)**

BULL TEMPLE ROAD, BENGALURU-560019

**DEPARTMENT OF ELECTRICAL AND ELECTRONICS ENGINEERING**

**2021-2022**


# CERTIFICATE

Certified that the project work entitled **“SMART ENERGY METER WITH HOME AUTOMATION”** carried out by **Ananya Chakravarthi (1BM18EE007), Sangeetha S Iyer (1BM18EE045), Sandeep V(1BM18EE068) and Prayag Sridhar(1BM18EE041)** a bonafide students of BMS College of Engineering in partial fulfillment for the award of degree of Bachelor of Engineering in Department of Electrical and Electronics Engineering of Visvesvaraya Technological University, Belagavi during the year 2021-2022. It is certified that all corrections/suggestions indicated for internal assessment have been incorporated in the report deposited in the departmental library.

The project report has been approved as it satisfies the academic requirements in respect of project work prescribed for the said degree.

|  |  |  |
| --- | --- | --- |
| Signature of the Guide  **(Dr. S Pradeepa)** | Signature of the HOD  **(Dr. A N Nagashree)** | Signature of the Principal  **(Dr. Muralidhara S)** |

|  |  |
| --- | --- |
| Name of the Examiners | Signature |
| 1. |  |
| 2. |  |



**BMS COLLEGE OF ENGINEERING**

**(Autonomous Institute, Affiliated to VTU)**

BULL TEMPLE ROAD, BENGALURU-560019

**DEPARTMENT OF ELECTRICAL AND ELECTRONICS ENGINEERING**

**2021-2022**

**BONAFIDE CERTIFICATE FROM THE SUPERVISOR**

Certified that this project entitled **“SMART ENERGY METER WITH HOME AUTOMATION” carried out by Ananya Chakravarthi (1BM18EE007), Sangeetha S (1BM18EE045), Sandeep V (1BM18EE068) and Prayag Sridhar (1BM18EE041),** who carried out under my supervision. This project work dissertation report was thoroughly scrutinized and corrected by me. All the corrections are incorporated by the students and the project report satisfies the academic requirements in respect of project work prescribed for the award of said degree. I duly certify the same.

Signature of the Guide

**(Dr, S Pradeepa)**

# DECLARATION

We hereby declare that the project work entitled “**SMART ENERGY METER WITH**

**HOME AUTOMATION**” submitted to BMS College of Engineering, is a record of an

original work done by us under the guidance of **Dr S. Pradeepa, Professor**, Department of Electrical and Electronics Engineering, BMS College of Engineering, Bengaluru and this project work is submitted in partial fulfillment of the requirements for the award of the degree of Bachelor of Engineering in Electrical and Electronics Engineering. The results embodied in this thesis have not been submitted to any other University or Institute for the award of any degree.

|  |  |
| --- | --- |
| **NAME** | **SIGNATURE** |
| Ananya Chakravarthi |  |
| Sangeetha S |  |
| Sandeep V |  |
| Prayag Sridhar |  |

### ABSTRACT

Due to the development and improvement of technology and embedded systems, human lives have become easier with the help of newly developed smart systems. These days, people are more interested in using the internet to control and observe different types of devices. Internet of things (IoT) creates an innovative evolution of the technology world with a new era of mature intelligence computing. IoT can be defined as the connection between many kinds of devices like smartphones, personal computers, and tablets to the internet, which brings in a very new kind of communicating between things and people and also between things themselves.

IoT has led to the evolution of electric devices and provided greater growth for smart homes to improve the standard of life. Over the last few years, the concept of a smart home has become interesting among consumers. There are tons of research done on home automation using IoT and one such research helped in developing a smart home system that provides high security and is cheaper in cost. This further led to the development of a system for power utilization using IoT in homes. In this system, they make use of image processing for monitoring human activities. A well-known renowned scientist designed a system that has the capability to control many household devices using GSM and Wi-fi.

In our project, we make use of home automation and energy monitoring system and the energy collected is then updated to the cloud. Arduino is used to collect energy values by taking in current and voltage values from the respective sensors. Using Controller ESP8266, the energy values calculated is updated to the cloud for every one hour. Servers are used for calculating total energy consumption by house hold appliances and the details are then sent to the users.

### ACKNOWLEDGMENTS

We would like to take this opportunity to express our heartful gratitude to ***Dr. S Pradeepa***, Professor, B.M.S.C.E for her constant guidance and support throughout the year which helped us to complete the project.

Our earnest thanks to **Dr. A.N Nagashree**, HOD, Department of Electrical and Electronics,

B.M.S.C.E for extending her support and providing her valuable suggestions.

We also deeply value the inputs provided by **Dr. C Lakshmi Narayana**, Professor, Department of Electrical and Electronics who helped us to improvise our work.

We would like to express our gratitude towards parents & members of **B.M.S College of Engineering** for their kind co-operation and encouragement which help me in completion of this project.

Our thanks and appreciations also go to fellow students in developing the project and people who have willingly helped us out with their abilities.

**TABLE OF CONTENTS**

|  |  |
| --- | --- |
| **TITLE** | **PAGE NUMBER** |
| **ABSTRACT** | **5** |
| **ACKNOWLEDMENT** | **6** |
| **TABLE OF CONTENTS** | **7** |
| **LIST OF FIGURES** | **8** |

|  |  |
| --- | --- |
| **CHAPTERS** | **PAGE NUMBER** |
| **CHAPTER-1: INTRODUCTION** | **9** |
| **CHAPTER-2: SMART ENERGY METER** | **10-18** |
| **CHAPTER-3: HOME AUTOMATION** | **19-25** |
| **CHAPTER-4: INTEGRATION OF SMART ENERGY METER AND HOME AUTOMATION** | **26-32** |
| **CHAPTER-5: RESULTS** | **33** |
| **CHAPTER-6: FUTURE SCOPE** | **33** |
| **CHAPTER-7: SOFTWARE TOOL USED** | **33** |
| **CHAPTER-8: REFERENCES** | **34** |

**LIST OF FIGURES**

|  |  |
| --- | --- |
| **FIGURES** | **PAGE NUMBER** |
| **FIGURE 1.1: HOME AUTOMATION** | **9** |
| **FIGURE 2.1: BLOCK DIAGRAM OF SMART ENERGY METER** | **10** |
| **FIGURE 2.2: CIRCUIT DIAGRAM OF SMART ENERGY METER** | **11** |
| **FIGURE 2.3: ENERGY METER WHEN UNITS ARE GREATER THAN 3** | **16** |
| **FIGURE 2.4: ENERGY METER WHEN UNITS ARE LESS THAN 3** | **17** |
| **FIGURE 2.5: SMART ENERGY METER WHEN UNITS IS EQUAL TO ZERO** | **18** |
| **FIGURE 3.1: BLOCK DIAGRAM OF HOME AUTOMATION** | **19** |
| **FIGURE 3.2: CIRCUIT DIAGRAM OF HOME AUTOMATION** | **20** |
| **FIGURE 3.3: LED CONTROL USING VIRTUAL TERMINAL(USER INPUT)** | **23** |
| **FIGURE 3.4: FAN/MOTOR CONTROL USING VIRTUAL TERMINAL(USER INPUT)** | **24** |
| **FIGURE 3.5: ALL LOADS TURN OFF WHEN WRONG USER INPUT IS IDENTIFIED** | **25** |
| **FIGURE 4.1: BLOCK DIAGRAM OF INTEGRATED CIRCUIT** | **26** |
| **FIGURE 4.2: CIRCUIT DIAGRAM OF INTEGRATED CIRCUIT** | **27** |

## INTRODUCTION

A Prepaid Smart meter is used to measure energy consumption. The Energy meter shows the amount of units consumed and the associated electrical parameters. The user can check their Power usage from anywhere and at any time interval. The concept of Home automation is used to Turn on/off the household appliances using relay and Arduino interfacing. This project aims at integrating the above systems to provide a comprehensive solution to human intervention and appliance mechanization. The objective of this system is to automate appliance functions using sensors and consequently use the smart meter to bill the consumption information. This dual system mainly aids elderly and the disabled to control their utility appliances at the touch of a button. It also aids in consumer-side communication by utilities and demand side management.

For better understanding of the individual systems and their integration, we have simulated it using the Proteus 8 Professional (Version 8.12) software and Arduino IDE. The integration of smart energy meter and home automation with the LCD Display gives rise to an active feedback loop between data from the smart energy meter, the consumer and the home automation feature.



FIGURE 1.1: HOME AUTOMATION

### SMART ENERGY METER

The Smart Energy Meter works by measuring the electrical current flow and voltage at regular intervals and then adding this up to calculate the power used in a certain time period. This information is then displayed on the LCD screen.

Smart meters differ from automated meter devices like it uses different technology, kind of information they measure. Smart meters give in-detail data than old devices and also give users access to meter's energy data usage. By doing this, you have the ability to have your energy usage under control by altering your usage habits.

Smart meters have the ability to assist customers to become more energy well-structured while offering sufficient understanding and opportunities to help save income on the electricity bill.

### BLOCK DIAGRAM




FIGURE 2.1: BLOCK DIAGRAM OF SMART ENERGY METER

### SPECIFICATIONS

1. Voltage Range for Arduino - 7-12 V
2. Operating frequency of Arduino UNO - 16 MHz (ATMEGA328)
3. Voltage Divider Circuit (load V measurement) - 100kΩ and 10kΩ
4. Current Sensor ACS712
5. 16x2 LCD Display
6. 5V DC Voltage, (This DC shift is added to the incoming voltage level so that the negative portion of the signal may be converted into positive.)

### CIRCUIT DIAGRAM


****

FIGURE 2.2: CIRCUIT DIAGRAM OF SMART ENERGY METER

### : CODE

#include<EEPROM.h> #include <LiquidCrystal.h>

LiquidCrystal lcd(2, 3, 4, 5, 6, 7); // lcd(7,6,5,4,3,2); int led;

#define pulsein 9

#define relay 8

#define sw 4

int sensitivity = 185;

int offsetvoltage = 2500;

float Voltage1 = A0; //Defining and initializing the voltage float Current1 = A1;

float I1 = 0; float V1 = 0; float power; float energy =0; float t;

float adc =0.00;

unsigned int pusle\_count=0; float units=0;

unsigned int rupees=0;

unsigned int temp=0,i=0,x=0,k=0;

//char str[70]

char flag1=0,flag2=0;

//String bal="";

void setup()

{

lcd.begin(16,2); Serial.begin(9600); pinMode(led, OUTPUT); pinMode(pulsein, INPUT); pinMode( sw , INPUT); pinMode(relay, OUTPUT); digitalWrite(pulsein, HIGH); digitalWrite(relay, HIGH); lcd.setCursor(0,0); lcd.print("Smart Energy Meter");

delay(2000); lcd.clear();

digitalWrite(led, LOW); lcd.clear(); EEPROM.write(1,40);

rupees=EEPROM.read(1);

}

void loop()

rupees=EEPROM.read(1); units=rupees/5.0; lcd.clear(); lcd.setCursor(0,0); lcd.print("Units:"); lcd.print(units); lcd.setCursor(0,1);

if (units<1)

{

lcd.print("Supply Cut!"); lcd.print("Meter off!!!"); exit(0);

}

if(rupees<15) lcd.print("LOW Balance:"); else

lcd.print("Balance:"); lcd.print(rupees); lcd.print(" "); delay(1000); lcd.clear();

energy=energy+(power\*t);

V1= ((analogRead(A0)\*(4.5/1023)\*60)); adc= ((analogRead(A1))/1024.00)\*5000; I1=(adc-2500 )/185;

lcd.setCursor(11,0); lcd.print("V="); lcd.print(V1); lcd.setCursor(0,0); lcd.print("I= "); lcd.print(I1); power=V1\*I1; lcd.setCursor(0,1); lcd.print("POWER="); lcd.print(power); lcd.setCursor(11,1); lcd.print("ENERGY="); lcd.print(energy); delay(1000);

lcd.print(" "); read\_pulse(); check\_status(); if(temp==1)

{

//decode\_message();

}

}

void read\_pulse()

if(digitalRead(pulsein))

{

if ((0.00<I1) &&(I1<2.00))

{

if(units<1){lcd.print("Supply Cut");}

else

{

units--; rupees=units\*5; t=4.00;

EEPROM.write(1,rupees); while(!digitalRead(pulsein));

//digitalWrite(led,LOW); delay(1000);

}

}

if ((2.00<I1) &&(I1<3.00))

{

if(units<1){ lcd.print("Supply Cut.");}

else

{

units--; rupees=units\*5; t=2.00;

EEPROM.write(1,rupees); while(!digitalRead(pulsein));

//digitalWrite(led,LOW); delay(1000);

}

}

if ((3.00<I1) &&(I1<4.00))

{

if(units<1){lcd.print("Supply Cut.");}

else

{

units--; rupees=units\*5; t=1.33;

EEPROM.write(1,rupees); while(!digitalRead(pulsein));

//digitalWrite(led,LOW); delay(1000);

}

}

if (I1>4.00)

{

if(units<1){}

else

{

units--; rupees=units\*5; t=1.00;

EEPROM.write(1,rupees); while(!digitalRead(pulsein)); delay(1000);

}

}

}

}

void check\_status()

{

if(rupees>15)

{

digitalWrite(relay, HIGH); flag1=0;

flag2=0;

}

if(rupees<=15 && rupees>=5)

{

lcd.setCursor(0,1);

message\_sent();

}

if(rupees<5 && flag1==0)

{

digitalWrite(relay, LOW); lcd.clear(); lcd.setCursor(0,1); lcd.print("Low Balance"); delay(2000);

lcd.clear();

lcd.print("Please Recharge!! "); lcd.setCursor(0,1); lcd.print("the Meter ");

//message\_sent(); flag1=1;

}

}

/\*

void decode\_message()

{

x=0,k=0,temp=0; while(x<i)

{

while(str[x]=='#')

{

x++;

bal=""; while(str[x]!='\*')

{

bal+=str[x++];

}

}

x++;

}

bal+='\0';

}

void message\_sent()

{

lcd.clear();

lcd.print("Please recharge!!"); delay(1000);

lcd.clear();

}

### 2.4 DESIGN AND ANALYSIS

**Case 1**: Initially when units is more than 3.





FIGURE 2.3: ENERGY METER WHEN UNITS ARE GREATER THAN 3

When units are greater than 3, LCD displays the amount of energy is being consumed along with Voltage, current, power and units remaining.

**Case 2:** When units is less than 3.







FIGURE 2.4: ENERGY METER WHEN UNITS ARE LESS THAN 3

When units are less than 3, a message **LOW BALANCE** is displayed and alerts the consumer to

**RECHARGE** with a message.

**Case 3:** When units is equal to 0





FIGURE 2.5: SMART ENERGY METER WHEN UNITS IS EQUAL TO ZERO

When unit goes to 0, the supply is cut off as the Relay circuit will switch to the other terminal. A message is sent to the consumer notifying that the supply is cut off

### HOME AUTOMATION

“Smart Home” or “Intelligent Home” refers to automation of home appliances based on sensor monitoring. These systems include centralized control and surveillance of lighting, security and temperature of appliances within a house. HAS’s enables energy efficiency, imbibing sustainability values in power consumption for users. The circuit is controlled by a number of sensors which activate the relays based on the threshold values and hence signals circuit operation. The LCD screen is used to display the status of the appliances..

The devices we have chosen for the circuit are bulbs, LED Lamps and Fan motors. The home automation system is one of the most useful features for the elderly and disabled. It provides increased security and simplicity with regard to power control and use.

### : BLOCK DIAGRAM


****

FIGURE 3.1: BLOCK DIAGRAM OF HOME AUTOMATION

### : CIRCUIT SPECIFICATIONS

* + 1. Operating frequency of ARDUINO UNO - 16 MHz (ATMEGA328)
    2. 16x2 LCD Display
    3. Relay
    4. BC547 NPN transistor
    5. Resistors(1k) , diodes
    6. LED 12V
    7. Motor- nominal voltage 12V
    8. Serial monitor, to use virtual terminal

### : CIRCUIT DIAGRAM


****

FIGURE 3.2: CIRCUIT DIAGRAM OF HOME AUTOMATION

### : CODE

#include <LiquidCrystal.h> // includes the LiquidCrystal Library LiquidCrystal lcd(2,3,4,5,6,7); // Creates an LCD object. Parameters:

//(rs, enable, d4, d5, d6, d7)

const int m1=10; const int m2=11; char NUM;

int F=0,R=0;

int N=0;

void setup() {

pinMode(8, OUTPUT); pinMode(13, OUTPUT); pinMode(9, OUTPUT); pinMode(m2, OUTPUT);

Serial.begin(9600); lcd.begin(16, 2);

lcd.clear(); lcd.setCursor(0, 0);

lcd.print("HOME AUTOMATION");

delay(5000); lcd.clear();

}

void loop() { if(Serial.available())

{

NUM= Serial.read();

if(NUM=='A')

{

digitalWrite(8,HIGH);

//delay(1000); lcd.clear(); lcd.setCursor(0, 0); lcd.print("LED ON");

}

else if(NUM=='B')

{

digitalWrite(8,LOW);

//delay(1000); lcd.clear(); lcd.setCursor(0, 0); lcd.print("LED OFF");

}

else if(NUM=='C')

{

digitalWrite(13,HIGH);

//delay(1000); lcd.clear(); lcd.setCursor(0, 0); lcd.print("FAN ON ");

}

else if(NUM=='D')

{

digitalWrite(13,LOW);

//delay(1000); lcd.clear(); lcd.setCursor(0, 0); lcd.print("FAN OFF");

}

else if(NUM=='E')

{

digitalWrite(9,HIGH);

//delay(1000); lcd.clear(); lcd.setCursor(0, 0);

lcd.print("MOTOR ON");

}

else if(NUM=='F')

{

digitalWrite(9,LOW);

//delay(1000); lcd.clear(); lcd.setCursor(0, 0);

lcd.print("MOTOR OFF");

}

else

{

digitalWrite(9,LOW); digitalWrite(13,LOW); digitalWrite(8,LOW); lcd.clear(); lcd.setCursor(0,0); lcd.print("ALL OFF"); delay(2000);


}

}

}

### 3.4: DESIGN AND ANALYSIS

**Case 1:** LED controls depends on serial input given by the user. When “A” is given as the input the led turns ON and when “B” is given as input the led turns OFF.







FIGURE 3.3: LED CONTROL USING VIRTUAL TERMINAL(USER INPUT)

**Case 2:** MOTOR/FAN control depends on serial input given by the user.

* When “C” is given as the input the FAN turns ON and when “D” is given as input the FAN turns OFF.
* When “E” is given as the input the MOTOR turns ON and when “F” is given as input the MOTOR turns OFF.






FIGURE 3.4: FAN/MOTOR CONTROL USING VIRTUAL TERMINAL(USER INPUT)

**Case 3:** LED/MOTOR/FAN control depends on serial input given by the user.

When the user gives any other input, then all the relay will turn down and all loads will TURN OFF.




FIGURE 3.5: ALL LOADS TURN OFF WHEN WRONG USER INPUT IS IDENTIFIED

### INTEGRATION OF SMART ENERGY METER AND HOME AUTOMATION

An integrated system of metering and control provides dual benefits of automation and billing. The project involves the concept of automating appliances, then bringing into picture- the smart metering which performs energy and power calculations. This provides mechanized control, preventing consumers from energy wastage and removing human intervention from the metering and billing areas.

In addition, we propose to imbibe data analytics features within the system to perform studies and give consumer reports on their usage pattern and suggest solutions based on thresholds

### : BLOCK DIAGRAM





FIGURE 4.1: BLOCK DIAGRAM OF INTEGRATED CIRCUIT

### : CIRCUIT DIAGRAM




FIGURE 4.2: CIRCUIT DIAGRAM OF INTEGRATED CIRCUIT

## : CODE

#include <EEPROM.h>

#include <LiquidCrystal.h>

/\* ---------- LCD pins (same as your Proteus drawing) --- \*/

LiquidCrystal lcd(2, 3, 4, 5, 6, 7);

/\* ---------- I/O pins ---------------------------------- \*/

constexpr byte RELAY\_PIN = 8; // cuts mains

constexpr byte PULSE\_PIN = 9; // 3200-imp/kWh LED, active-LOW

constexpr byte LOAD\_LED\_PIN = 10; // serial 'A/B'

constexpr byte LOAD\_FAN\_PIN = 11; // serial 'C/D'

constexpr byte VOLTAGE\_PIN = A0; // divider ~0-4.5 V

constexpr byte CURRENT\_PIN = A1; // ACS712 ~0-5 V

/\* ---------- Wi-Fi & Adafruit IO ----------------------- \*/

#include <AdafruitIO\_WiFi.h>

AdafruitIO\_WiFi io(IO\_USERNAME, IO\_KEY, WIFI\_SSID, WIFI\_PASS);

AdafruitIO\_Feed \*feedPower = io.feed("power");

AdafruitIO\_Feed \*feedUnits = io.feed("units");

AdafruitIO\_Feed \*feedBalance = io.feed("balance");

/\* ---------- Meter / tariff constants ----------------- \*/

constexpr float ADC\_mV\_STEP = 5000.0 / 1023.0; // mV per LSB

constexpr float VOLTAGE\_GAIN = 60.0 \* 4.5 / 1023.0;

constexpr float CURR\_ZERO\_mV = 2500.0;

constexpr float CURR\_SENS\_mV\_A = 185.0;

constexpr uint8\_t EEPROM\_BAL\_ADDR = 1;

constexpr uint8\_t DEFAULT\_RUPEES = 40; // 8 units (₹5 each)

constexpr float RS\_PER\_UNIT = 5.0;

constexpr uint8\_t LOW\_BALANCE\_RS = 15;

float vRms = 0, iRms = 0, pInst = 0, energyWh = 0;

/\* ---------- Timing ----------------------------------- \*/

constexpr unsigned long SAMPLE\_MS = 1000;

constexpr unsigned long ADAFRUIT\_MS = 30000;

unsigned long tLastSample = 0;

unsigned long tLastPublish = 0;

bool lastPulse = HIGH; // for edge detect

/\* ===================================================== \*/

void setup() {

Serial.begin(9600);

lcd.begin(16, 2);

pinMode(RELAY\_PIN, OUTPUT);

pinMode(LOAD\_LED\_PIN, OUTPUT);

pinMode(LOAD\_FAN\_PIN, OUTPUT);

pinMode(PULSE\_PIN, INPUT\_PULLUP);

// init balance once

if (EEPROM.read(EEPROM\_BAL\_ADDR) == 0xFF)

EEPROM.write(EEPROM\_BAL\_ADDR, DEFAULT\_RUPEES);

lcd.print(F("Connecting WiFi"));

io.connect(); // blocks until connected

lcd.setCursor(0, 1); lcd.print(F("Adafruit IO OK"));

delay(1500);

showBalance();

tLastSample = millis();

tLastPublish = millis();

}

/\* ===================================================== \*/

void loop() {

io.run(); // keep MQTT link alive (non-blocking)

/\* ------------ Serial load control ------------------ \*/

if (Serial.available()) {

switch (Serial.read()) {

case 'A': digitalWrite(LOAD\_LED\_PIN, HIGH); break;

case 'B': digitalWrite(LOAD\_LED\_PIN, LOW); break;

case 'C': digitalWrite(LOAD\_FAN\_PIN, HIGH); break;

case 'D': digitalWrite(LOAD\_FAN\_PIN, LOW); break;

}

}

/\* ------------ 1 s acquisition ---------------------- \*/

if (millis() - tLastSample >= SAMPLE\_MS) {

tLastSample += SAMPLE\_MS;

acquireVI(); // updates vRms, iRms, pInst

energyWh += pInst \* (SAMPLE\_MS / 3600000.0);

lcd.setCursor(0, 0);

lcd.print(F("P:"));

lcd.print(pInst, 0);

lcd.print(F("W "));

lcd.print(F("E:"));

lcd.print(energyWh, 1);

lcd.print(F("Wh "));

handlePulse();

checkBalance();

}

/\* ------------ Adafruit IO publish ------------------ \*/

if (millis() - tLastPublish >= ADAFRUIT\_MS) {

tLastPublish += ADAFRUIT\_MS;

sendToAdafruit();

}

}

/\* ==================== helpers ======================== \*/

void acquireVI() {

int rawV = analogRead(VOLTAGE\_PIN);

int rawI = analogRead(CURRENT\_PIN);

vRms = rawV \* VOLTAGE\_GAIN;

float mV = rawI \* ADC\_mV\_STEP;

iRms = (mV - CURR\_ZERO\_mV) / CURR\_SENS\_mV\_A;

if (iRms < 0) iRms = 0;

pInst = vRms \* iRms;

}

void handlePulse() {

bool now = digitalRead(PULSE\_PIN);

if (lastPulse == HIGH && now == LOW) { // falling edge

deductOneUnit();

sendToAdafruit(); // instant update

}

lastPulse = now;

}

void deductOneUnit() {

uint8\_t bal = EEPROM.read(EEPROM\_BAL\_ADDR);

if (bal >= RS\_PER\_UNIT) bal -= RS\_PER\_UNIT;

else bal = 0;

EEPROM.write(EEPROM\_BAL\_ADDR, bal);

energyWh = 0; // reset counter

showBalance();

}

void checkBalance() {

uint8\_t bal = EEPROM.read(EEPROM\_BAL\_ADDR);

if (bal == 0) {

digitalWrite(RELAY\_PIN, LOW);

lcd.setCursor(0, 1);

lcd.print(F("SUPPLY CUT "));

} else if (bal < LOW\_BALANCE\_RS) {

lcd.setCursor(0, 1);

lcd.print(F("Low Bal Rs: "));

lcd.print(bal);

lcd.print(F(" "));

digitalWrite(RELAY\_PIN, HIGH);

} else {

digitalWrite(RELAY\_PIN, HIGH);

}

}

void showBalance() {

uint8\_t bal = EEPROM.read(EEPROM\_BAL\_ADDR);

lcd.clear();

lcd.setCursor(0, 0);

lcd.print(F("Units: "));

lcd.print(bal / RS\_PER\_UNIT, 1);

lcd.setCursor(0, 1);

lcd.print(F("Bal Rs: "));

lcd.print(bal);

lcd.print(F(" "));

}

/\* ---------- Adafruit IO publish helper --------------- \*/

void sendToAdafruit() {

if (io.status() != AIO\_CONNECTED) return; // don’t block

uint8\_t bal = EEPROM.read(EEPROM\_BAL\_ADDR);

float unitsLeft = bal / RS\_PER\_UNIT;

feedPower ->save(pInst);

feedUnits ->save(unitsLeft);

feedBalance->save(bal);

}

**4.4 THE HARDWARE MODEL OF THE CIRCUIT**

A circuit board with lights and wires

AI-generated content may be incorrect.

A circuit board with wires and lights

AI-generated content may be incorrect.

A close-up of a device

AI-generated content may be incorrect.

## RESULTS

* **Smart energy meters** measure electricity consumed and display it to the user. Home

**automation** will monitor/control home appliances.

* Both have a common underlying principle - encouraging **savings** in consumption. Hence, an energy meter which has an interface for home automation can switch off home appliances when not in use.
* This project has thus proposed an IOT based energy efficient practical system integrating mechanization in common utilities. The concept involves metering without human intervention and sensor based automation of appliances.
* The project would hence serve as an extensive use to the elderly and the disabled, providing ease of accessibility and insight.

## FUTURE SCOPE:

* Utilising the LCD details to create a report for energy consumption of a

consumer, thereby allowing the consumer to fine-tune his/her consumption pattern.

* Extending home automation features to Temperature, alarm and motion sensing.
* Hardware implementation of Integrated system with above features

## SOFTWARE TOOLS USED

* Proteus 8
* ARDUINO ID

## REFERENCES:

1. R. T. Mathew, S. Thattat, K. V. Anirudh, V. P. K. Adithya and G. Prasad, "Intelligent Energy Meter with Home Automation," 2018 3rd International Conference for Convergence in Technology (I2CT), 2018, pp. 1-4, doi: 10.1109/I2CT.2018.8529702.
2. W. Hlaing, S. Thepphaeng, V. Nontaboot, N. Tangsunantham, T. Sangsuwan and C. Pira, "Implementation of WiFi-based single phase smart meter for Internet of Things (IoT)," 2017 International Electrical Engineering Congress (iEECON), 2017, pp. 1-4, doi: 10.1109/IEECON.2017.8075793.
3. H. V. Bhatnagar, P. Kumar, S. Rawat and T. Choudhury, "Implementation model of Wi-Fi based Smart Home System," 2018 International Conference on Advances in Computing and Communication Engineering (ICACCE), 2018, pp. 23-28, doi: 10.1109/ICACCE.2018.8441703.
4. International Journal of Engineering Research & Technology (IJERT) ISSN: 2278-0181 Published by, [www.ijert.org](http://www.ijert.org/) NCETESFT - 2020 Conference Proceedings
5. B. K. Barman, S. N. Yadav, S. Kumar and S. Gope, "IOT Based Smart Energy Meter for Efficient Energy Utilization in Smart Grid," 2018 2nd International Conference on Power, Energy and Environment: Towards Smart Technology (ICEPE), 2018, pp. 1-5, doi: 10.1109/EPETSG.2018.8658501.
6. H. Das and L. C. Saikia, "GSM enabled smart energy meter and automation of home appliances," 2015 International Conference on Energy, Power and Environment: Towards Sustainable Growth (ICEPE), 2015, pp. 1-5, doi: 10.1109/EPETSG.2015.7510071.
7. Abdulla AlHammadi, Aisha AlZaabi, Bashayer AlMarzooqi, Suhail AlNeyadi, Zayed AlHashmi, Maad Shatnawi, "Survey of IoT-Based Smart Home Approaches", Advances in Science and Engineering Technology International Conferences (ASET) 2019, pp. 1-6, 2019